<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">unw\_dyn\_region\_info\_t:

        - insn_count can be negative to indicate that the region is
          at the end of the procedure; in such a case, the negated
          insn_count value specifies the length of the final region
          in number of instructions.  There must be at most one region
          with a negative insn_count and only the last region in a
          procedure's region list may be negative.  Furthermore, both
          di-&gt;start\_ip and di-&gt;end\_ip must be valid.
</pre></body></html>